Freeze Frame Settings group

Freeze Frame decides when, how often and how long the holographic signal will freeze. This decision is somewhat random and creates the effect of a signal loss.

NOTE: A frozen frame in an amination is difficult to show in a still image manual, so there are no sample images to accompany the descriptions on this page.

At left, the Freeze Frame settings. At right, the Freeze Frame checkbox.

% Chance of Freeze Frame

Determines possibility of a random Freeze Frame. Default setting is 10%. Value range is 0 to 100, measured in percentage. Higher values increase the possibility of a frozen frame.

Freeze Duration

Sets the amount of time for a Freeze Frame. Default setting is 0.3. Value range is 0 to 5, measured in seconds. Higher values increase the length of the freeze.

Random Duration Variation (%)

Determines how much a block of Freeze Frame time can vary in length. Default setting is 25%. Value range is 0 to 100, measured in percentage. Higher values increase the variation in length.