## Linux gamecon.c

### Notes

- You can only use true switch-based joysticks with this circuit.
- PPJoy, unlike Linux, will not allow you to use this interface on the same parallel port as another interface type.
- The pull-up resistors are 10k Ohm.
- The original diagram only specifies "Power"; we source it from Pin 1 (nStrobe). PPJoy drives pin 1, 14, 16 and 17 high; any one of these can be used as power source.
- General notes about interface construction

### Credits

The original diagram and information for this interface can be found at http://www.charmed.com/support/kernel/docs/joystick-parport.txt.