## DirectPad Pro SNES interface

Controller | Parallel Port
--- | ---
Pad 1 | Pad 2 | Pad 3 | Pad 4 | Pad 5
Power | +5v
Clock | 2
Latch | 3
Data | 10 | 12 | 13 | 15 | 11
Ground | 18

### Notes

- This interface is exactly the same as the SNESKey interface.
- This interface is the same as the Linux SNES interface, except for the numbering of of the pads.
- General notes about interface construction
- This interface supports configurable timing parameters - see Changing timing parameters on how to change these values and SNES/NES timing parameters for their meanings.

### Credits

The original diagram and information for this interface can be found at http://www.arcadecontrols.com/Mirrors/www.ziplabel.com/dpadpro/snes.html.

SNESKey documentation and diagrams can be found at http://www.arcadecontrols.com/Mirrors/www.csc.tntech.edu/~jbyork/manual/manual.html