[Manufacturer Datasheet]
NUMBER OF CELLS NS=36
MAXIMUM POWER PMAX=60
VOLTAGE AT PMAX=17.1
CURRENT AT PMAX=3.5
OPEN-CIRCUIT VOLTAGE VOC=21.1
SHORT-CIRCUIT CURRENT ISC=3.8
TEMPERATURE COEFF. OF VOC=-0.38
TEMPERATURE COEFF. OF ISC=0.065
SD LIGHT INTENSITY S0=1000
SD TEMPERATURE TREF=25
DV/DI (SLOPE) AT VOC=-0.68
[Model Parameters (defined)]
BAND ENERGY EG=1.12
IDEALITY FACTOR A=1.2
SHUNT RESISTANCE RSH=1000
COEFFICIENT KS=0
[Model Parameters (calculated)]
SERIES RESISTANCE RS=0.008
SHORT CIRCUIT CURRENT ISC0=3.8
SATURATION CURRENT IS0=2.16e-008
TEMPERATURE COEFFICIENT CT=0.00247
[Operating Conditions]
LIGHT INTENSITY S=1000
AMBIENT TEMPERATURE TA=25
