<module>
No description
</module>
<name> IRpad IR,
</name>
<member> linkinterface_IRreceive receive receive,

</member>,
<member> var_uint16 OS_EventFlag OS_EventFlag,

</member>,
<member> event receive_event ReceiveEvent,

</member>,
<member> event nodata_event NodataEvent,

</member>,
<member> event NUMBER_event NUMBEREvent,

</member>,
<member> event CH_event CHEvent,

</member>,
<member> event CH0_event CH0Event,

</member>,
<member> event CH1_event CH1Event,

</member>,
<member> event PREV_event PREVEvent,

</member>,
<member> event NEXT_event NEXTEvent,

</member>,
<member> event PLAY_event PLAYEvent,

</member>,
<member> event EQ_event EQEvent,

</member>,
<member> event VOL0_event VOL0Event,

</member>,
<member> event VOL1_event VOL1Event,

</member>,
<member> event A100_event A100Event,

</member>,
<member> event A200_event A200Event,

</member>,
<member> var_int32 data KeyData,

</member>,
<member> var_uint16 OS_time OS_time,

</member>,
<member> function_void OS_init OS_init,

</member>,
<member> function_void OS_run OS_run,

</member>,
<member> const_int32 NONE NONE,
</member>,
<member> const_int32 NUM0 NUM0,

</member>,
<member> const_int32 NUM1 NUM1,

</member>,
<member> const_int32 NUM2 NUM2,

</member>,
<member> const_int32 NUM3 NUM3,

</member>,
<member> const_int32 NUM4 NUM4,

</member>,
<member> const_int32 NUM5 NUM5,

</member>,
<member> const_int32 NUM6 NUM6,

</member>,
<member> const_int32 NUM7 NUM7,

</member>,
<member> const_int32 NUM8 NUM8,

</member>,
<member> const_int32 NUM9 NUM9,

</member>,
<member> const_int32 CH0 CH0,

</member>,
<member> const_int32 CH CH,

</member>,
<member> const_int32 CH1 CH1,

</member>,
<member> const_int32 PREV PREV,

</member>,
<member> const_int32 NEXT NEXT,

</member>,
<member> const_int32 PLAY PLAY,

</member>,
<member> const_int32 VOL0 VOL0,

</member>,
<member> const_int32 VOL1 VOL1,

</member>,
<member> const_int32 EQ EQ,

</member>,
<member> const_int32 A100 A100,

</member>,
<member> const_int32 A200 A200,

</member>,
