

		IN1.D0_OUT = 0;
		KeyList.11(bit) = OUT1.D0_IN;
		KeyList.0(bit) = OUT2.D0_IN;
		KeyList.10(bit) = OUT3.D0_IN;
		IN1.D0_OUT = 1;
		
		IN2.D0_OUT = 0;
		KeyList.9(bit) = OUT1.D0_IN;
		KeyList.8(bit) = OUT2.D0_IN;
		KeyList.7(bit) = OUT3.D0_IN;
		IN2.D0_OUT = 1;
		
		IN3.D0_OUT = 0;
		KeyList.6(bit) = OUT1.D0_IN;
		KeyList.5(bit) = OUT2.D0_IN;
		KeyList.4(bit) = OUT3.D0_IN;
		IN3.D0_OUT = 1;
		
		IN4.D0_OUT = 0;
		KeyList.3(bit) = OUT1.D0_IN;
		KeyList.2(bit) = OUT2.D0_IN;
		KeyList.1(bit) = OUT3.D0_IN;
		IN4.D0_OUT = 1;
		
		
		
		