public link unit receive {}
driver.receive = receive;
public link bit OS_EventFlag = driver.OS_EventFlag;
public link bit 按键值 = driver.data;
public link bit OS_time = driver.OS_time;
public link void OS_init(){} = driver.OS_init;
public link void OS_run(){} = driver.OS_run;
public link bit 无按键按下 = driver.NONE;
public link bit 数字0 = driver.NUM0;
public link bit 数字1 = driver.NUM1;
public link bit 数字2 = driver.NUM2;
public link bit 数字3 = driver.NUM3;
public link bit 数字4 = driver.NUM4;
public link bit 数字5 = driver.NUM5;
public link bit 数字6 = driver.NUM6;
public link bit 数字7 = driver.NUM7;
public link bit 数字8 = driver.NUM8;
public link bit 数字9 = driver.NUM9;
public link bit 电源键 = driver.POWER;
public link bit 菜单键 = driver.MENU;
public link bit TEST键 = driver.TEST;
public link bit 音量加 = driver.VOLINC;
public link bit 返回键 = driver.RETURN;
public link bit 前一个 = driver.PRE;
public link bit 播放键 = driver.PLAY;
public link bit 后一个 = driver.NEXT;
public link bit 音量减 = driver.VOLDEC;
public link bit C键 = driver.C;
