public link bit OS_time = driver.OS_time;
public link bit Rvalue = driver.Rvalue;
public link bit Gvalue = driver.Gvalue;
public link bit Bvalue = driver.Bvalue;
public link bit RCvalue = driver.RCvalue;
public link bit GCvalue = driver.GCvalue;
public link bit BCvalue = driver.BCvalue;
public link void OS_init(){} = driver.OS_init;
public link void OS_run(){} = driver.OS_run;
public link void SetWhite0(){} = driver.set_white0;
public link void SetWhite(bit n1,bit n2,bit n3){} = driver.set_white;
