<module>
No description
</module>
<name> IRpad1 ir,
</name>
<member> linkinterface_IRreceive receive receive,

</member>,
<member> var_uint16 OS_EventFlag OS_EventFlag,

</member>,
<member> event receive_event receive_event,

</member>,
<member> event nodata_event nodata_event,

</member>,
<member> event POWER_event POWER_event,

</member>,
<member> event MENU_event MENU_event,

</member>,
<member> event TEST_event TEST_event,

</member>,
<member> event RETURN_event RETURN_event,

</member>,
<member> event VOLINC_event VOLINC_event,

</member>,
<member> event VOLDEC_event VOLDEC_event,

</member>,
<member> event PRE_event PRE_event,

</member>,
<member> event NEXT_event NEXT_event,

</member>,
<member> event PLAY_event PLAY_event,

</member>,
<member> event C_event C_event,

</member>,
<member> event NUMBER_event NUMBER_event,

</member>,
<member> var_int32 data key_data,

</member>,
<member> var_uint16 OS_time OS_time,

</member>,
<member> function_void OS_init OS_init,

</member>,
<member> function_void OS_run OS_run,

</member>,
<member> const_int32 NONE NONE,
</member>,
<member> const_int32 NUM0 NUM0,

</member>,
<member> const_int32 NUM1 NUM1,

</member>,
<member> const_int32 NUM2 NUM2,

</member>,
<member> const_int32 NUM3 NUM3,

</member>,
<member> const_int32 NUM4 NUM4,

</member>,
<member> const_int32 NUM5 NUM5,

</member>,
<member> const_int32 NUM6 NUM6,

</member>,
<member> const_int32 NUM7 NUM7,

</member>,
<member> const_int32 NUM8 NUM8,

</member>,
<member> const_int32 NUM9 NUM9,

</member>,
<member> const_int32 POWER POWER,

</member>,
<member> const_int32 MENU MENU,

</member>,
<member> const_int32 TEST TEST,

</member>,
<member> const_int32 VOLINC VOLINC,

</member>,
<member> const_int32 RETURN RETURN,

</member>,
<member> const_int32 PRE PRE,

</member>,
<member> const_int32 PLAY PLAY,

</member>,
<member> const_int32 NEXT NEXT,

</member>,
<member> const_int32 VOLDEC VOLDEC,

</member>,
<member> const_int32 C C,

</member>,
