public link bit OS_time = driver.OS_time;
public link bit OS_EventFlag = driver.OS_EventFlag;
public const int32 PWM周期 = 0;
driver.TT = PWM周期;
public link void OS_init(){} = driver.OS_init;
public link void 设置PWM周期为_(bit n1){} = driver.set_t;
public link void OS_thread(){} = driver.OS_thread;
public link void OS_run100us(){} = driver.OS_run100us;
public link void OS_run(){} = driver.OS_run;
public link void OS_ClearWatchDog(){} = driver.OS_ClearWatchDog;
public link void 指示灯点亮(){} = driver.LightOpen;
public link void 指示灯熄灭(){} = driver.LightClose;
public link void 指示灯反转(){} = driver.LightSwap;
public link void 指示灯闪烁_次(bit n1){} = driver.LightFlashTimes;
public link void 指示灯闪烁(){} = driver.LightFlash;
