
GPD Win joystick upgrade instructions


1, let the device shutdown (not restart)

2, hold down the keyboard R3 button, press the power button to boot, waiting for the screen display release R3

3, enter the system after the joystick into the upgrade mode, joystick and mouse function will temporarily failure

4, run "HJM1954M Updater V20 20161216.exe" program

  
Update Firmware can click on the state, click Update Firmware to complete the upgrade.

Note: the handle did not enter the upgrade mode update Firmware is gray non clickable state, please try again the above upgrade method

Note：

1, improve the corresponding speed button,

2, optimize the mouse movement speed

3, optimize the response speed of the left mouse joystick

4, increase the mouse mode L3 as the left mouse button, R3 as the right mouse button

The difference between V22 and V23 is that the V23 mouse does not accelerate.