# Inverter

Bibliothek: | Base
Eingeführt: | 2.0 Beta 1
Aussehen: |
Shaped: |
Rectangular: |

## Verhalten

The NOT Gate emits the complement of whatever input it receives. The truth table for a NOT gate is the following.

x | out
--- | ---
0 | 1
1 | 0

If the input is unspecified (i.e., floating), then the output will also be unspecified - unless the "Gate Output When Undefined" option is "Error for undefined inputs," in which case the output is an error. If the input is an error value, then the output will also be.

A multi-bit NOT gate will perform the above transformation bitwise on its input.

## Pins (wenn das Bauelement nach Osten zeigt)

West edge (input, bit width according to Data Bits attribute)
  The component's input.
East edge (output, bit width according to Data Bits attribute)
  The output, whose value is the complement of the input value.

## Attribute

When the component is selected or being added, Alt-0 through Alt-9 alter its Data Bits attribute and the arrow keys alter its Facing attribute.

Ausrichtung
  Die Richtung des Bauelements (Lage des Ausgangs im Vergleich zum Eingang).
Data Bits
  The bit width of the component's input and output.
Gate Size
  Determines whether to draw a larger or a smaller version of the component.
Label
  The text within the label associated with the gate.
Label Font
  The font with which to render the label.

## Verhalten des Schaltwerkzeugs

Keines.

## Verhalten des Textwerkzeugs

Allows the label associated with the gate to be edited.

Zurück zur Bibliotheksreferenz