# Demultiplexer

Bibliothek: | Auswahlschaltungen
Eingeführt: | 2.0 Beta 11
Aussehen: |

## Verhalten

Copies the input on the west edge onto exactly one of the outputs on the east edge; which of these outputs is specified via the current value received through the input on the south edge. I find it useful to think of a demultiplexer as analogous to a railroad switch, controlled by the select input.

(Incidentally, some authorities spell this demultiplexor, but demultiplexer is the predominant spelling.)

## Pins (wenn das Bauelement nach Osten zeigt)

West edge (input, bit width matches Data Bits attribute)
  The value to be routed to one of the outputs on the east edge.
East edge, variable number (outputs, bit width matches Data Bits attribute)
  The outputs are numbered starting with 0 on the north. An output will match the west input if its number matches the value currently received through the select input on the south; otherwise, its value will be either all-zeroes or all-floating, depending on the value of the Three-State? attribute. If the select input contains any unspecified bits, then all outputs are floating.
South edge (input, bit width matches Select Bits attribute)
  Select input: The value of this input determines to which output on the east edge to route the value received on the west edge.

## Attribute

When the component is selected or being added, the digits '1' through '4' alter its Select Bits attribute, Alt-0 through Alt-9 alter its Data Bits attribute, and the arrow keys alter its Facing attribute.

Ausrichtung
  The direction of the component (specifying which side has the outputs).
Auswahlleitungen
  The bit width of the component's select input on its south edge. The number of outputs for the demultiplexer will be 2selectBits.
Data Bits
  The bit width of the data being routed through the demultiplexer.
Three-state?
  Specifies whether the unselected outputs should be floating (Yes) or zero (No).

## Verhalten des Schaltwerkzeugs

Keines.

## Verhalten des Textwerkzeugs

Keines.

Zurück zur Bibliotheksreferenz