## STFormat

### Notes

- It is not recommended to build this interface. Rather build Amiga4Player. This interface can be turned into the Amiga4Player interface by moving the Joystick 1 pin 6 (fire) connection from pin 1 (nStrobe) to pin 13 (Select) on the Parallel Port.
- It is doubtful if this interface will properly work on any PC parallel port - the fire button on joystick 1 will not function properly
- General notes about interface construction

### Credits

The original diagram and information for this interface can be found at http://www.umich.edu/~archive/atari/Misc/4plradap.txt.