<module>
无线遥控器, 当用户按键时就会触发 <按键按下事件>, 用户可以在事件处理代码中读取按键值进行处理, 比如控制小车前进后退等. 当按键松开时就会触发 <按键松开事件>
</module>
<name> Pack 遥控器,
</name>
<member> linkinterface_IRreceive receive receive,

</member>,
<member> var_uint32 OS_EventFlag OS_EventFlag,

</member>,
<member> event key0_press_event □键按下时,

</member>,
<member> event key0_up_event □键松开时,

</member>,
<member> event key1_press_event ×键按下时,

</member>,
<member> event key1_up_event ×键松开时,

</member>,
<member> event key2_press_event ○键按下时,

</member>,
<member> event key2_up_event ○键松开时,

</member>,
<member> event key3_press_event △键按下时,

</member>,
<member> event key3_up_event △键松开时,

</member>,
<member> event key4_press_event R1键按下时,

</member>,
<member> event key4_up_event R1键松开时,

</member>,
<member> event key5_press_event L1键按下时,

</member>,
<member> event key5_up_event L1键松开时,

</member>,
<member> event key6_press_event R2键按下时,

</member>,
<member> event key6_up_event R2键松开时,

</member>,
<member> event key7_press_event L2键按下时,

</member>,
<member> event key7_up_event L2键松开时,

</member>,
<member> event key8_press_event 左方向键按下时,

</member>,
<member> event key8_up_event 左方向键松开时,

</member>,
<member> event key9_press_event 下方向键按下时,

</member>,
<member> event key9_up_event 下方向键松开时,

</member>,
<member> event key10_press_event 右方向键按下时,

</member>,
<member> event key10_up_event 右方向键松开时,

</member>,
<member> event key11_press_event 上方向键按下时,

</member>,
<member> event key11_up_event 上方向键松开时,

</member>,
<member> event key12_press_event 开始键按下时,

</member>,
<member> event key12_up_event 开始键松开时,

</member>,
<member> event key13_press_event 右摇杆按下时,

</member>,
<member> event key13_up_event 右摇杆松开时,

</member>,
<member> event key14_press_event 左摇杆按下时,

</member>,
<member> event key14_up_event 左摇杆松开时,

</member>,
<member> event key15_press_event 选择键按下时,

</member>,
<member> event key15_up_event 选择键松开时,

</member>,
<member> var_uint16 OS_time OS_time,

</member>,
<member> function_void OS_init OS_init,

</member>,
<member> function_void OS_run OS_run,

</member>,
